Documentation Camel V1

tags: camel, camel V1

1. Fichier de configuration json

Configuration avec communication radio en LoRa:

{ "rtc_type": "am1805", "time_between_measures_s": 600, "number_measures_before_write_sd": 18, "number_writes_in_interval_file": 8, "lora_active": true }

Configuration sans communication radio:

{ "rtc_type" : "am1805", "time_between_measures_s" : 600, "number_measures_before_write_sd" : 18, "number_writes_in_interval_file" : 8, "lora_active" : false }

2. Manuel utilisateur

camelv1_user_manual_fr.pdf

3. Javascript Codec to decode LoRaWAN frames

The function used to parse the bytes transmitted in LoRaWAN