Pinout of the Flipper

tags : flipper, nrf52, pinout, schematic

1. Description

Pinout Documentation generated with Graphical Datasheets

2. Top Side Pinout

WARNING !! There is a mistake on the pin naming : XLB connector is 2×10 pins, XLB_10 does not exist on the right side

flipper_top.svg

3. Bottom Side Pinout

Warning !! this pinout view must be use with care, according to the silkscreen on the PCB, the pin NAME are right but the side is wrong !! pin 1 of the header is at the bottom right corner (not at left as in the pinout view)